**For Immediate Release**

**New Kinetex Plank, Strata, Combines Modern, Nature-Inspired Aesthetic with Superior Comfort and Durability**

*Grainy Rock-Like Appearance in Distinctive 18” x 36” Tile Format Resembles Hard Surface Look*

CHICAGO—NEOCON EXPO (SHOWROOM #10-118), JUNE 13, 2016 –

J+J Flooring Group’s new Kinetex plank, Strata, seamlessly marries a nature-inspired aesthetic with a thoughtfully designed pattern in a 18” x 36” format. The result is a fresh, modern-looking flooring option resembling a classic hard surface appearance that brings multiple design installation opportunities.

As a textile composite flooring, Strata offers all the advantages of a soft surface product, including superior slip and rolling resistance, improved acoustics and anti-fatigue benefits.

The indigenous beauty of sedimentary rocks layered over time is at the heart of Strata’s design inspiration. Its organic pattern achieves a grainy, rock-like appearance that cleverly alludes to the look of stone slab. Available in nine neutral colorways, Strata is a functional and highly flexible flooring solution. Its sophisticated and unobtrusive design is perfect for a variety of end-use environments.

J+J engaged noted flooring designer Karen Maffetone of Karen Maffetone LLC., to lead the development of Strata.

As with all Kinetex products, Strata contains the warmth and feel of a soft surface, but with the high performance attributes of hard surface. Constructed of knitted polyester fabric and cushioned polyester felt backing, it is one of the most slip resistant flooring surfaces ever tested, wet or dry, thus reducing the potential for slip and fall injuries. Its unique low profile also has minimal rolling resistance, further mitigating possible injuries from pushing and pulling. It has one of the highest Noise Reduction Coefficients (NRC) and Impact Insulation Classifications (IIC) rating of any commercial flooring product, resulting in dramatic reductions in both airborne and structure borne noise. Its unique construction and materials composition provides the ability to reduce repetitive foot stress injuries and injuries related to walking frequently from place to place.

Strata comes standard with J+J’s innovative pre-applied releasable adhesive, Pre-Fix™. Fully integrated with the unique Kinetex backing, this meticulously designed system allows for an increased adhesive performance while also offering a highly breathable tile which can be installed on concrete with RH levels up to 99 percent.

Strata is made with Universal Fibers, a 100 percent solution dyed polyester fiber that provides rich, long lasting color with superior stain resistance and wear performance.

Kinetex products contribute to sustainable design. They have a 50 percent lower environmental impact than traditional hard or soft surface flooring. They also contain 55 percent recycled content, are fully closed-loop recyclable and certified to NSF 140 Platinum. All Kinetex products meet the Carpet & Rug Institute’s Green Label Plus certification for low indoor air emissions and come with a third-party Environmental Product Declaration

For information, visit [www.jjflooringgroup.com](http://www.jjflooringgroup.com) or call 800.241.4586.

###

About Kinetex

All Kinetex products are constructed of knitted polyester fabric and cushioned polyester felt backing. The result is a soft textile aesthetic with the durability of hard surface flooring. Kinetex provides superior stain and crushing resistance through its ability to withstand more than 5 million foot traffics. It also provides better acoustics, comfort, cleanliness and slip-and-fall resistance than traditional hard surface flooring. Kinetex’s lifecycle cost of ownership (flooring materials, installation and maintenance over 7-10 years) is less than rubber, LVT and VCT flooring.

Named one of *Environmental Building News’* Top 10 Green Building Products of 2014, Kinetex has 50 percent lower environmental impact than traditional hard or soft surface flooring. Kinetex products contain 55 percent recycled content, are fully closed-loop recyclable and are certified to NSF 140 Platinum. All Kinetex products meet the Carpet & Rug Institute’s Green Label Plus certification for low indoor air emissions and come with a third-party Environmental Product Declaration.

**About J+J Flooring Group**

Established in 1957, J+J Flooring Group is a leading manufacturer of commercial specified flooring.  With our two brands - Invision broadloom and modular carpet and Kinetex textile composite flooring - we provide a range of product and service solutions to meet the needs of our customers in the corporate workplace, education, healthcare, retail and hospitality sectors.

In 2016, J+J Flooring Group joined Engineered Floors, LLC. Based in Dalton, Ga., Engineered Floors is a privately held carpet producer founded in 2010 by Robert E. Shaw. The company, which employs more than 2,800 people, produces stain-resistant and colorfast solution dyed nylon and polyester fiber and carpeting for residential replacement, new home builder, multi-family and main street commercial applications. To learn more visit, [www.engineeredfloorsllc.com.](http://www.engineeredfloorsllc.com/index.php)

Media Contacts:

Matt Spaulding

Spaulding Communications

404.270.1010 ext. 1

[matts@spauldingcommunications.com](mailto:matts@spauldingcommunications.com)

Natalie Faulkner

Director of Marketing Communications

J+J Flooring Group

800.241.4586 ext. 8311

[natalie.faulkner@jjflooringgroup.com](mailto:natalie.faulkner@jjflooringgroup.com)